The versions of Licel software that you have downloaded are not compatible with LabView versions older than 6.0!

To install the newest Licel Bore Sight Alignment software, do the following three steps.

1. Backup all your current Licel software libraries, in case you want to restore them, by either
compressing them (Zip, ARJ, TAR, etc...) or burning them onto CD.

2. Scan your disks to find all the versions of the following files and directories and delete them once you
have made backups of them
    1. BoreAnalysis.llb
    2. BoreLive.llb
    3. BorePulse.llb
    4. BoreRemoteControl
    5. GCS_Q-Motion
    6. LicelFile
    7. LicelModule.llb
    8. LicelTCPIP.llb
    9. LicelTCPIP_API.llb
   10. LicelTCPIP_Apps.llb
   11. LicelUtil.llb
   12. Picomotor_8742_Drive_dll
   13. Search Controllers.llb
   14. BoreDrive.llb
   15. Newport.llb
   16. NewportSMC100.llb
   17. Picomotor8742.llb
   18. QMotion_E872.llb

3. Unpack the files in TREthernet.zip to the desired directory.

After that you should be able to run all the files.  If you are still having problems, try
doing a mass compile on the directory where the software was extracted to.  Please note that
step 2 is a necessity, since LabView often links to various libraries with the same name.  As
a result, if a library is installed twice, one can not be certain which library is actually
being used.

If you still have problems, please contact Licel for further instructions.

Licel GmbH
Gustav-Meyer-Allee 52
13355 Berlin
Germany

email: info@licel.com
web:    www.licel.com
Phone: +49-30-283 91737
Fax: +49-30-283 91738
