<?xml version="1.0"?>
<nidocument>
<nicomment>
<nifamily familyname="Licel-Errors" displayname="Licel error codes">
</nifamily>
</nicomment>
<nierror code="-10401" LicelSource="HS-Licel Initialize DIO card.vi">
Licel HS_50+: Check if the DIO 32 board is correctly mounted, that the DAQ driver version is installed correctly, and that the board is registered at the Measurement and Automation Explorer.
</nierror>
<nierror code="5001" LicelSource="Postan.llb\data analysis (a+p).vi">
Licel HS_50+/TCPIP: Check the data types of the signals you are about to analyze.
</nierror>
<nierror code="5010" LicelSource="Postan.llb\analog to photoncounting.vi">
Licel HS_50+/TCPIP: Warning - Make sure that you are operating with an appropriate signal range.
</nierror>
<nierror code="5011" LicelSource="Postan.llb\analog to photoncounting.vi">
Licel HS_50+/TCPIP: Warning - Make sure that you are operating with an appropriate signal range.
</nierror>
<nierror code="5012" LicelSource="Postan.llb\analog to photoncounting.vi">
Licel HS_50+/TCPIP: Warning - Make sure that you are operating with an appropriate signal.
</nierror>
<nierror code="5700" LicelSource="HS-Licel Wait For Ready.vi">
Licel HS_50+: Internal warning code for timeout indication.
</nierror>
<nierror code="5800" LicelSource="Licel TCPIP  Wait For Ready.vi">
Licel TCPIP: Internal warning code for timeout indication.
</nierror>
<nierror code="5801" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the syntax of the command.
</nierror>
<nierror code="5802" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: An unknown command was sent to the controller. Please check the firmware version and the availability of the command
</nierror>
<nierror code="5803" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The password sent to the controller with the TCPIP command is wrong.
</nierror>
<nierror code="5804" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Please check the old password, that both new passwords are equal, and that the new password has a non-zero length.
</nierror>
<nierror code="5805" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The WHITELIST command was not accepted. Please check for the correct password and if the syntax of the allowed hosts IP addresses / address ranges are correct.
</nierror>
<nierror code="5806" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The password sent to the controller with the ACCESS command is wrong or the command syntax is not correct.
</nierror>
<nierror code="5807" LicelSource="Licel Module Check CAPs Error.vi">
Licel Module: The Licel Ethernet Controller has not the capabilities to support the software module
</nierror>
<nierror code="5808" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The TCP/IP buffer could not be dumped probably because somebody continous to write. 
</nierror>
<nierror code="5810" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The parameter sent with the RANGE command must be in the range between 0 and 2 (inclusive).
</nierror>
<nierror code="5811" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The parameter sent with the DISCRIMINATOR command must be in the range between 0 and 63 (inclusive).
</nierror>
<nierror code="5812" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check if a TR with the requested device number is installed and correctly set up.
</nierror>
<nierror code="5813" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the connection with the TR identified by the requested device number.
</nierror>
<nierror code="5814" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the cable connection with the TR identified by the requested device number. Contact Licel in case of further error messages of this type.
</nierror>
<nierror code="5815" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The timeout parameter sent with the MWAIT command must be in the range between 0 and 400 (inclusive).
</nierror>
<nierror code="5816" LicelSource="Licel TCPIP Select Device.vi">
Licel TCPIP Select: Please make sure that the desired device number is in range.
</nierror>
<nierror code="5820" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The PUSH command cannot be executed because the controller runs in the MPUSH mode.
</nierror>
<nierror code="5821" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The MPUSH command cannot be executed because the controller runs in the PUSH mode.
</nierror>
<nierror code="5822" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Carefully check the syntax of the MPUSH command.
</nierror>
<nierror code="5823" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The Number of Shots set by the PUSH and/or MPUSH commands must be in the range between 0 and 14 (inclusive)
</nierror>
<nierror code="5824" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the network configuration for the push socket.
</nierror>
<nierror code="5825" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The command is not available when either the PUSH mode or MPUSH mode is active.
</nierror>
<nierror code="5826" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check that the controller and the TR support shot numbers up to 64k
</nierror>
<nierror code="5827" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check that the controller and the TR support shot numbers up to 64k
</nierror>
<nierror code="5830" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Verify that the PMT you tried to access does exist and is correctly connected to the controller.
</nierror>
<nierror code="5831" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Verify that the APD you tried to access does exist and is correctly connected to the controller.
</nierror>
<nierror code="5832" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Verify that the Battery you tried to access does exist and is correctly connected to the controller.
</nierror>
<nierror code="5833" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Verify that the Device you tried to access does exist and is correctly connected to the controller.
</nierror>
<nierror code="5834" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The APDs can be supplied by batteries only if all batteries are connected with their supply pins.
</nierror>
<nierror code="5835" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: The batteries can be connected with their charge pins only if no APD uses them as supply.
</nierror>
<nierror code="5836" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the syntax and number of parameters sent with the APDC command.
</nierror>
<nierror code="5838" LicelSource="Control APD-PMT Check APD-Battery Switches.vi">
Licel TCPIP: An illegal combination of Battery Connectors and APD Supplies has been detected. Please check the hardware setup.
</nierror>
<nierror code="5839" LicelSource="Control APD-PMT Switch APD Supply Mode.vi">
Licel TCPIP: The APD supply mode could not be set or unset. Please check the hardware setup.
</nierror>
<nierror code="5841" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the syntax of the CLOUD command.
</nierror>
<nierror code="5842" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Enable Cloud detection before sending the SKY? command.
</nierror>
<nierror code="5851" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the command syntax of the TRIGGERMODE command
</nierror>
<nierror code="5852" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Check the command syntax of the TRIGGERTIME command
</nierror>
<nierror code="5855" LicelSource="Licel TCPIP Set Trigger Timing.vi">
Licel TCPIP: Make sure that the laser is running and that it's trigger out (Q-Switch out) is correctly wired to the trigger input of the timing controller.
</nierror>
<nierror code="5857" LicelSource="Set Trigger Rabbit Parameters.vi">
Licel TCPIP: Check the syntax of the command
</nierror>
<nierror code="5860" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Please check that both signal and background ranges, and that the start bin of the first defined range, and the bin interval between both ranges  do not exceed 1023.
</nierror>
<nierror code="5861" LicelSource="Licel TCPIP Generate Error.vi">
Licel TCPIP: Please check the number of bins and cycles
</nierror>
<nierror code="5900" LicelSource="TCPIP Live Diplay TCPIP.vi">
Licel TCPIP Live Display: A marker error occurred while attempting to read pushed data.
</nierror>
<nierror code="5910" LicelSource="ControlAPD-PMT CleanUpDetectorTR_Assignment.vi">
TR-Detector Assignment: compare DetectorTR_Assignment.ini with the indicated backup file.
</nierror>
<nierror code="5911" LicelSource="ControlAPD-PMT HandlePMT_Error.vi">
Check the PMT calibration, contact Licel for support
</nierror>
<nierror code="5920" LicelSource="TCPIP_Pulse ReadPHD_FromTextFile.vi">
Make sure that the selected file is a valid pulse height distribution file.
</nierror>
<nierror code="6510" LicelSource="Licel Module Run Module Initialize.vi">
The initialization process of the module took longer than the specified timeout value.
</nierror>
<nierror code="6511" LicelSource="Licel Module Wait Notification.vi">
Check wether the vi associated with the module is broken. Run the vi stand-alone to search for eventually missing sub-vis.
</nierror>
<nierror code="6512" LicelSource="Licel Module Stop Module Wait.vi">
Check the initialization/stop/exit sequence of the module. 
</nierror>
<nierror code="6520" LicelSource="Licel Module Set Signal Bool.vi">
Check if such a boolean control exists and that it is placed directly on the front panel. 
</nierror>
<nierror code="6800" LicelSource="Boresite Alignment.vi">
The motors did not stop after a time of 20 seconds. Please check the motors.
</nierror>
<nierror code="6840" LicelSource="LWSMC100_Licel MergeSMC100Error.vi">
Check the communication with the controller.
</nierror>
<nierror code="9001" LicelSource="LicelTCPIP_API_ClientCore GenerateError.vi">
Carefully check the TCP/IP API command that has been sent and the reply by the API.
</nierror>
<nierror code="13001" LicelSource="M_Acquis WaitTCPIP_HandlerNotifications.vi">
Make sure that all instances of M-Acquis TCPIP Handler.vi are alive
</nierror>
<nierror code="13002" LicelSource="M_Acquis TCPIP_HandlerNotificationHandler.vi">
Make sure that the correct command has been send to all instances of M-Acquis TCPIP Handler.vi
</nierror>
<nierror code="13003" LicelSource="M_Acquis CancelTCPIP_HandlerNotifiers.vi">
Make sure that the last notofication has been cancelled after receiving it.vi
</nierror>
<nierror code="13010" LicelSource="various">
A netCDF variable ID could not be found due to one of the following reasons: a) the netCDF properties have nor correctly been read from the netCDF file or b) the requested variable is not included in the netCDF properties or c) an error occurred while processing a netCDF ID cluster
</nierror>
<nierror code="13100" LicelSource="Licel CDFUtil Call ncgen.vi">
This error was reported by netgen.exe. Make sure that your current version is correct. Refer to the details returned by netgen.exe.
</nierror>
<nierror code="13101" LicelSource="Licel CDFUtil Generate Error.vi">
This error was reported by netcdf.dll. Please make sure that the function calls are correctly submitted. Refer to the netCDF error code.
</nierror>
<nierror code="13201" LicelSource="Licel Module Find Initialization File.vi">
Please make sure that the requested initialization file contains at least the correct load description to run the application.
</nierror>
<nierror code="13202" LicelSource="LicelModule CopyTempSubModule.vi">
The input is not a file.
</nierror>
<nierror code="13210" LicelSource="LicelModule InitializeModuleErrorHandler.vi">
Check the Licel Main.ini (or the used derivate's initialization file).
</nierror>
<nierror code="13301" LicelSource="LicelTCPIP_API WaitQueueResponse.vi">
Check the source code 
</nierror>
<nierror code="13302" LicelSource="LicelTCPIP_API ParseBuffer.vi">
Check the source code 
</nierror>
<nierror code="13303" LicelSource="LicelTCPIP_API ParseBuffer.vi">
Check the source code 
</nierror>
<nierror code="17013" LicelSource="HS32-Licel Check Task IDs.vi">
Please make sure that the indicated initialization file contains the correct load descriptions for the application.
</nierror>
<nierror code="424242" LicelSource="LicelFile LogUsedVersion.vi">
This is a logging entry for the used version
</nierror>
<nierror code="1073479938" LicelSource="HS-Licel Reset.vi">
Licel HS_50+: Reset not supported.
</nierror>
<nierror code="1073479939" LicelSource="HS-Licel Self Test.vi">
Licel HS_50+: Self-test not supported.
</nierror>
<nierror code="1073479941" LicelSource="HS-Licel Revision Query.vi">
Licel HS_50+: Revision Query not supported
</nierror>
</nidocument>